For Windows Developer

1.Please check files in the SDK directory.

2.ZLDToupCamSetup.exe is the DirectShow/TWAIN SDK package. Running it will install the driver, DirectShow/TWAIN files, sample application and its source code.

3.ToupCam.zip is a Native C/C++ SDK for developer, including the demo application and documents for reference.

4. About the driver installation, driver validation and deletion operation, please read ToupCamDriverInstallValidationDeletion.pdf file in the ToupViewHelpManual directory.


///////////////////////////////////////////////////////////////////////////////////////
For Linux Uesr

Untar ToupLiteLinux.tgz anywhere on your hard drive. For arch x86, unstar ToupLite-1.0-x86.tgz. For arch x64 untar ToupLite-1.0-x64.tgz. Run the run file will install the application. Root privilege is needed during installation. Double click ToupLite on the Desktop to run the application.

/////////////////////////////////////////////////////////////////////////////////////
For Mac User

Copy the dmg file anywhere on your hard drive. Double click the ToupLiteOSX.dmg file and it will mount automatically. Drag the ToupLite.app to the Application folder to install the application. Double click ToupLite.app to run the application.

/////////////////////////////////////////////////////////////////////////////////////
For Android User

Install ToupView.apk on your Android devices and this will work with wifi cameras.